Tesoro Technology USA Inc.

Language:

Welcome to TESORO World |

Congratulations on purchasing your very own TESORO LOBERA™ Full Color Illumination Gaming Keyboard - a gaming keyboard engineered to suit the needs of every gamer. Featuring Gaming grade mechanical switches(SUPREME) and full color whole zone illumination, it is the keyboard of choice for optimizing the gaming experience.

Switchable USB 6 N-Key/ Full N-Key Rollover
Gaming grade mechanical key switch
Gaming grade 50 million key actuations
3 thumb keys for instant macro launch
Instant 5 profiles shift keys
512Kbit onboard memory
5 profiles, full key programmable
Instant Record button under Game Mode
6 levels LED backlight/dimming & Game Zone control
Full color whole zone illumination

F/W and application on-line update
User friendly UI for macro setup
Gold-plated USB connector
Embedded multimedia keys
2 High speed USB 2.0 ports
Audio headphone and microphone jacks
DC-IN jack (5V 2.5A) for additional power supply
Anti-slip design rubberized tilt feet
Compatible with Windows XP/Vista/7/8

Operating System |

The software supports the following operating systems:
| Windows XP 32 bits
| Windows XP 64 bits
| Windows Vista 32 bits
| Windows Vista 64 bits
| Windows 7 32 bits
| Windows 7 64 bits
| Windows 8 32 bits
| Windows 8 64 bits

Installation |

Step 1 | Plug TESORO LOBERA™ Full Color Illumination Gaming Keyboard into the USB, PHONE (green), MIC (pink) port of
| your computer.
Step 2 | Download LOBERA Software from the Tesoro website.
Step 3 | Click the "setup.exe", the setup instruction will guide you through the setup process; click finish button to restart your computer.
Step 4 | TESORO icon will be displayed on the lower right taskbar when completed.
To get more help or profile macro keys setup for TESORO LOBERA, please run the application program and click "TESORO LOGO" at the top
right-hand corner, or visit TESORO LOBERA product pages at www.tesorotec.com
Registering your TESORO LOBERA™
Visit www.tesorotec.com for online product registration:
One year limited manufacture warranty
Free online technical support

Instruction |

| Software Overview |

|  |  | Profile tab selection
|  |  | Import your configuration file
|  |  | Export your configuration file
|  |  | Save setting to current profile
|  |  | Save the current profile and close software window
|  |  | Reset current profile to default configuration
|  |  | Memory space display
|  |  | Key indicator display
|  |  | Minimize software window
|  |  | Close software
|  |  | Launch help file
|  |  | Macro setting window
|  |  | Assign single key to different single key
|  |  | Assign single key to launch the program
|  |  | AP will auto-switch to PF1 ~PF5 when specific program launched
|  |  | Assign single key to disable
|  |  | Assign single key to default
|  |  | Open thumb key setting window

| Operation Guide |

Macro Key Setting

Step 1
To configure your LOBERA™ application program, simply open “LOBERA” file or double click the gaming keyboard iconat bottom right task bar.
Step 2
Select “Profile 1” or other profiles which you wish to configure.
Step 3
Click the selected key on the virtual keyboard screen, the selected key will change to purple color
Step 4
Click on Macro setting , enter the Marco setting window.
Step 5
Click on Start Record button to start recording Macro keys
Step 6
Click on Stop Record button to complete the record process
Step 7
Click Stop Record button to end recording. Then click “APPLY” to save Macro setting or click to save Macro and exit

Other functions' description as below:
|  | Start Recording Marco Keys.
|  | Stop Recording.
|  | Adjust key sequence to move down.
|  | Adjust key sequence to move up.
|  | Delete Key item.
|  | Set key stroke’s Delay timing. Move cursor and select the key stroke’s timer area on the right side. Fill required delay timing in text box, then click DELAY button. Key stroke’s Delay timing will be changed
|  | Select macro Repeat mode
|  | Save current setting to marco file

Step 8
After click , a confirm window will appear. Click “YES” to save current setting to profile

Step 9
After you finish all keys' setting. Click to save current profile and continue to set other profiles.
Step 10
After click , a confirm window will appear. Click “YES” to save current setting to profile.

Step 11
Wait and finish Macro Setting.

Now you've completed the macro setting, enjoy and have fun ! |